FLAC3D Gitbook

Kyeong Sun Kim

Table of Contents

# 1 KAIST Model


## 1.1 Initial Configuration


import itasca as it  
import numpy as np  
np.set\_printoptions(threshold=20)  
it.command("python-reset-state false")  
from itasca import zonearray as za  
from itasca import gridpointarray as gpa  
  
# PARAMETERS #  
  
\_D\_shaft = 1  
\_H\_shaft = 7.45  
\_T\_plate = 1.5  
\_B\_footing = 3.25  
\_D\_footing = \_H\_shaft + \_T\_plate  
\_B\_soil = \_B\_footing\*5  
\_D\_soil = \_D\_footing+3  
  
\_radial = 50  
\_perimeter = 2\*\_radial  
\_axial = 2\*\_radial  
\_outer = 2\*\_radial  
  
\_bulk = 13.9e9  
\_shear = 10.4e9  
  
\_E\_o = 1e7  
\_const = 1e8  
\_poisson = 0.25

## 1.2 Zones



# ZONE #  
command\_zone = """  
model new  
z crea r-t p 0 (0,0,0) ...  
 p 1 ({B\_soil},0,0) ...   
 p 2 (0,{D\_soil},0) ...  
 p 3 (0,0,{B\_soil}) ...  
 p 4 ({B\_soil},{D\_soil},0) ...  
 p 5 (0,{D\_soil},{B\_soil}) ...  
 p 6 ({B\_soil},0,{B\_soil}) ...  
 p 7 ({B\_soil},{D\_soil},{B\_soil}) ...  
 p 8 ({B\_footing},0,0) ...  
 p 9 (0,0,{B\_footing}) ...  
 p 10 ({B\_footing},{D\_soil},0) ...  
 p 11 (0,{D\_soil},{B\_footing}) ...  
 p 12 ({B\_footing},0,{B\_footing}) ...  
 p 13 ({B\_footing},{D\_soil},{B\_footing}) ...  
 size {radial} {axial} {perimeter} {outer} ...  
 rat 1 1 1 1.01 ...  
 fill  
"""  
  
command = command\_zone.format(  
B\_footing = \_B\_footing,  
B\_soil = \_B\_soil,  
D\_soil = \_D\_soil,  
radial=\_radial,  
axial = \_axial,  
perimeter = \_perimeter,  
outer = \_outer)  
  
it.command(command)





## 1.3 Group

# GROUP #  
p = za.pos()  
x,y,z = p.T  
print(it.zone.count(), "zones in whole model")  
  
shaft = reduce(np.logical\_and, (np.sqrt(x\*\*2+z\*\*2)<\_D\_shaft, y<\_H\_shaft))  
za.set\_group(shaft, "shaft") # set the zones with shaft = true have "shaft" and "geometry"  
print(za.in\_group("shaft").sum(), "zones in shaft group.") #output how many zones are in the corner group  
  
plate = reduce(np.logical\_and, (x<\_B\_footing,z<\_B\_footing, y>\_H\_shaft,y<\_D\_footing))  
za.set\_group(plate, "plate") # set the zones with plate = true have "plate" and "geometry"  
print(za.in\_group("plate").sum(), "zones in plate group.") #output how many zones are in the corner group

## 1.4 Constitutive Model

Besides standard looping as depicted above, one can easily loop over sets of model objects (i.e., zones, gridpoints, structural element nodes, etc.) using the loop foreach construct. In this case, a container of objects must be given by a FISH intrinsic such as zone.list. A practical use of the loop foreach construct is to install a nonlinear initial distribution of elastic moduli in a FLAC3D grid. Suppose that the Young’s modulus at a site is given by this equation:


where z is the depth below surface, and c and E∘ are constants. We write a FISH function to install appropriate values of bulk and shear modulus in the grid, as in this example:


# CONSTITUTIVE MODEL  
it.command("""  
zone cmodel assign elastic range group "Radial Tunnel1"  
zone cmodel assign elastic range group 'shaft'  
zone cmodel assign elastic range group 'plate'  
  
fish define fname(E\_o,const)  
loop foreach pnt zone.list  
z\_depth = zone.pos.y(pnt)  
E = E\_o+const\*math.sqrt(z\_depth)  
zone.prop(pnt,'young')=E  
end\_loop  
end  
@fname({E\_o\_},{const\_})  
zone property poisson {poisson\_}  
plot item create zone contour property name 'young'  
""".format(E\_o\_=\_E\_o,const\_=\_const,poisson\_=\_poisson))  
  
it.command("""  
zone property bulk {bulk} shear {shear} range group 'shaft'  
zone property bulk {bulk} shear {shear} range group 'plate'  
""".format(bulk=\_bulk,shear=\_shear))

Again, you can verify correct operation of the function by printing or plotting shear and bulk moduli.

In the function install, the loop takes place over all zones in the global list of zones. The FISH statement loop foreach is a variation of the loop statement that sets pnt to each zone in zone.list. Inside the loop, the z-coordinate of each zone centroid is used to calculate the Young’s modulus, given in the equation above. We assume that the datum (or ground surface reference point) is at z = 0. The variables zone.pos.z(pnt) and zone.prop(pnt, ‘young’) are zone intrinsics. (Recall that we talked about the gridpoint intrinsic gp.force.unbal earlier.) Here, we set properties directly from within a FISH function, rather than with a zone property command as in an earlier example.

# SOFTENING MODEL #  
#it.command("""  
#zone cmodel assign strain-softening range group "Radial Tunnel1"  
#zone property density 2500 bulk 2e8 shear 1e8 range group "Radial Tunnel1"  
#zone property cohesion 2e6 friction 45 tension 2e5 dilation 10 range group "Radial Tunnel1"  
#zone property table-friction 'fri' table-cohesion 'coh' table-dilation 'dil' range group "Radial Tunnel1"  
#table 'fri' add (0, 45) (.05, 42) (.1, 40) (1, 40)  
#table 'coh' add (0,2e6) (.05,1e6) (.1,5e5) (1,5e5)   
#table 'dil' add (0, 10) (.05, 3) (.1, 0)  
#""")





## 1.5 Soil-Structure Interface

# INTERFACE

## 1.6 Boundary Conditions

## 1.7 Initial Equilibrium

## 1.8 Alterations

## 1.9 Results

# 2 Axial Concrete Pile



## 2.1 Problem Description

### 2.1.1 Problem Statement

The pile is subjected to an axial load of 100 kN, and then the top of the pile is moved horizontally for a displacement of 4 cm. The goal is to determine relation of axial loading to the ultimate bearing capacity. And, lateral load-deflection curve is calculated.

1. origin at the top of the pile, z upward.
2. z=0: free surface
3. z=-8: fixed in z-eirection
4. x=+8, -8, y = 8: roller
5. skin friction is modeled by placing an interface between pile concrete wall and clay. In it, fric angle of 20 and c=30kPa are assumed.
6. toe interface is placed between pile tip and clay *note: Zone faces are separated in a previous command so that the gridpoints common to both will be separated as well.*  
   *note: include Figure of grid (geometry)*

### 2.1.2 Main Parameters

Diameter = 0.6 m  
Length = 5  
Clay  
GWT = 5.5m

## 2.2 Modeling Procedure

1. equil. stress state under gravity load before install.  
   1-1) water table is created at z=5.5  
   1-2) wet density of clay is assigned below this water table.
2. equil. stress state after installation.  
   2-1) change properties of pile zones from those  
   representing clay to those representing concrete.  
   2-2) vertical equil. stress distribution at this equil. state is shown in  
   *note: include Figure of contours of vertical stress at ini state incld. pile weight*
3. apply vertical velocity at top of pile  
   “ramp” = boundary condition is increased linearly  
   *note: critical timestep is controlled by high stiffness of concrete*  
   If velocity is sudden, inertial effects will dominate and renders difficulty to identification of steady state response of system  
   table “ramp” is used to apply velocity to pile top gridpoints.  
   *note: FISH FUNCTION vert\_load calculates axial stress at the top of pile and stores value as a history*  
   For efficiency, gridpoints on cap surface are stored in symbol “cap” as a map  
   *note: include plot of axial stress vs axial displ. at pile toe. ramp = (0,5e-8), step number = 30000*  
   *note: combined damping is used to remove kinetic energy for prescribed loading condition. This is because mass-adjustment process depends on velocity sign-changes..*  
   *note: FISH FUNCTION tot\_reac monitors soil reaction along pile as a func of lateral displ. tot\_reac creates tables of soil reaction (p) vs. lateral displ (y) at diff. locations along pile to generate p-y curve.*  
   *note: include Figure of p-y curve at 11 equidistant points along pile*

## 2.3 Zones

model new  
model title 'Axial and lateral loading of a concrete pile'  
; create grid interactively from the extruder tool,   
; exported to geometry.f3dat from State Record pane.  
call 'geometry' suppress  
zone generate from-extruder  
; Reflect the grid to get a 1/2 space instead of a 1/4 space  
zone reflect dip-direction 270 dip 90

## 2.4 Groups

; Name intersections of things named in the two extruder views  
zone group 'clay' range group 'clay-c' or 'clay-s' or 'wetclay-s'  
zone group 'pile' range group 'pile-c' group 'pile-s' or 'remove-s'  
zone group 'remove' range group 'remove-s' group 'pile-c' not ;   
zone face group 'wall' internal range group 'wall-c' group 'pile'  
zone face group 'base' internal range group 'base-s' group 'pile'  
zone face skin ; Name far field boundaries  
; Delete the area marked for removal  
zone delete range group 'remove'  
;  
; setup interfaces  
; separate using zone separate  
; all at once so common nodes are separated  
zone separate by-face new-side group 'iwall' slot 'int' ...  
 range group 'wall' or 'base'  
; Want two different interfaces for proper normal direction at corner  
zone interface 'side' create by-face range group 'wall' and 'iwall'  
zone interface 'base' create by-face range group 'base' and 'iwall'  
; Save initial geometric state  
model save 'geometry'

## 2.5 Properties

; Initialize gravity, pore-pressures, density, and stres state  
model gravity 10  
; water table information  
zone water density 1000  
zone water plane origin (0,0,-5.5) normal (0,0,-1)  
zone initialize density 1230  
zone initialize density 1550 range group 'wetclay-s' ; Wet density  
; assign properties to the soil and interfaces - temporarily remove pile cap  
zone cmodel assign mohr-coulomb ...  
 range group 'clay'  
zone property bulk 8.333e7 shear 3.846e7 cohesion 30000 fric 0 ...  
 range group 'clay'  
zone cmodel assign elastic range group 'pile'  
zone property bulk 8.333e7 shear 3.846e7 range group 'pile'  
zone cmodel assign null range group 'remove-s'  
zone interface 'side' node property stiffness-normal 1e8 ...  
 stiffness-shear 1e8 friction 20 cohesion 30000  
zone interface 'base' node property stiffness-normal 1e8 ...  
 stiffness-shear 1e8 friction 20 cohesion 30000

## 2.6 B.C. and I.C.

; boundary and initial stress conditions  
zone face apply velocity-normal 0 range group 'Bottom'  
zone face apply velocity-normal 0 range group 'East' or 'West'  
zone face apply velocity-normal 0 range group 'North' or 'South'  
zone initialize-stress ratio 0.4286  
zone interface 'side' node initialize-stresses  
zone interface 'base' node initialize-stresses

## 2.7 Initial Equilibrium

; Solve to initial equilibrium  
zone ratio local  
model solve ratio 1e-4  
model save 'initial'

## 2.8 Alterations

### 2.8.1 install the pile

; install the pile  
model restore 'initial'  
zone cmodel assign elastic range group 'pile'  
zone property bulk 13.9e9 shear 10.4e9 density 2500 range group 'pile'  
model solve ratio 1e-4  
model save 'install'

### 2.8.2 vertical loading

; vertical loading  
zone initialize state 0  
zone gridpoint initialize displacement (0,0,0)  
zone gridpoint initialize velocity (0,0,0)   
table 'ramp' add ([global.step],0) ([global.step+30000],-5e-8) ...  
 ([global.step+58000],-5e-8) ; Increase velocity applied to pile  
 ; over 30,000 steps  
zone face apply velocity-normal 1 table 'ramp' range group 'Top'  
history interval 250  
zone history name 'disp' displacement-z position (0,0,0)  
call 'load'  
fish history name 'load' @vert\_load  
zone mechanical damping combined  
model step 58000  
model save 'vertical-loading'

### 2.8.3 vertical then lateral loading

; vertical loading then lateral loading  
model restore 'install'  
zone initialize state 0  
zone gridpoint initialize displacement (0,0,0)  
zone gridpoint initialize velocity (0,0,0)   
zone face apply stress-zz [-1.0e5/(math.pi\*0.3\*0.3)] range group 'Top'  
model solve ratio 1e-4  
model save 'lateral-load-start'  
  
; apply lateral loading as x-velocity on cap  
zone initialize state 0  
zone gridpoint initialize displacement (0,0,0)  
zone gridpoint initialize velocity (0,0,0)   
zone face apply velocity-x 1e-7 range group 'Top'  
zone history name 'disp' displacement-x position 0,0,0  
call 'p-y' suppress ; Calculates p-y curve for pile, when tot\_reac is called  
@make\_pydata ; Generate p-y curve calculation data   
@output\_structure ; Sanity check of p-y curve data   
fish history name 'load' @tot\_reac  
model step 416500  
model save 'lateral-load'



# 3 Pull-Tests

 ## Problem Description *note: FISH function force is used to sum the raction forces and monitor nodal displacement generated by the pull-test*  
*note: free length of bolt that extends out of block + larger diameter*  
Perfectly plastic behavior of grout = max cohesion is exceeded +post-peak weakening of shear bond strength  
*note: bond strength softening of the grout is defined with keyword coupling-cohesion-table (see Rockbolt Behavior)*  
The relation btw shear disp. and cohesion weakening is prescribed  
thru table cct. softening of friction of grout canbe defined using keyword coupling-friction-table.

## 3.1 Zones

; ==================================================================  
; Simulation of pull-test for grouted reinforcement  
; using modified pile elements - Softening of cohesion  
; ==================================================================  
model new   
fish automatic-create off  
model title 'Pull-test using modified pile elements - cohesion softening'  
; Create a single rock block and set its material properties.  
zone create brick size 4 4 6 point 1 (0.4,0,0) point 2 (0,0.4,0) ...  
 point 3 (0,0,0.6)

## 3.2 Properties

zone cmodel assign elastic  
zone property bulk 5e9 shear 3e9  
zone face apply velocity-normal 0.0 range position-z 0.6  
; Create a pile element and assign properties  
struct pile create by-line (0.2,0.2,0.1) (0.2,0.2,0.7) segments 12  
struct pile property rockbolt-flag on  
struct pile property young 200e9 poisson 0.25 cross-sectional-area 5e-4 ...  
 perimeter 0.08  
struct pile property tensile-yield 2.25e5 ; ultimate tensile strength  
struct pile property moi-y 2.0e-8 moi-z 2.0e-8 moi-polar 4.0e-8 ; 0.25\*pi\*r^4  
struct pile property coupling-cohesion-shear 1.75e5 ...  
 coupling-stiffness-shear 1.12e7  
struct pile property coupling-cohesion-normal 1.75e5 ...  
 coupling-stiffness-normal 1.12e7  
struct pile property coupling-cohesion-table 'cct'  
; change in cohesion with relative shear displacement  
table 'cct' add (0,1.75e5) (0.025,1.75e4)

## 3.3 Initial Equilibrium

struct node fix velocity-x range position-z 0.7  
struct node initialize velocity-x 1e-6 local range position-z 0.7  
call 'pileforce' suppress ; FISH function calculates reaction force on zones

## 3.4 Alterations

; Set up histories for monitoring model behavior  
history interval 10  
fish history name 'force' @force  
struct node history name 'disp' displacement-z position (0.2,0.2,0.7)  
; Achieve a total displacement of 4.0 cm  
model cycle 40000  
;  
model save 'pull-5'

## 3.5 Some other notes

2.3. pull test with confinement “Pulltest06.f3dat” +modified pile logic.(see Behavior of Shear Coupling Springs) linear law is implemented.whereby reinforcement shear strength is defined as constant  
*(coupling-cohesion-shear)+ effective pressure*perimeter*fric angle(coupling-friction-shear)*  
This pressure dependence is activated automatically by issuing reinforcement properties(perimeter) and

2.5. pull test with tensile rupture “Pulltest08.f3dat” *note: tensile-yield, tensile-failure-strain: for limiting axial yield force and limiting axial strain for rockbolt*

# 4 Grid

## 4.1 Primitive Shapes







*note: zone create generates primitive grid*  
*note: zone gridpoint create puts gridpoints at specific locations*   
*note: zone gridpoint merge ensures separate primitives are connected properly*  
*note: zone attach connects primitive meshes of different zone sizes.*

zone create radial-cylinder size 5 10 6 12 fill  
zone create radial-cylinder size 5 10 6 12 ratio 1 1 1 5  
each size is controlled by a ratio (geometric ratio of 1.2 times preceding zone)

ex) 5 along innder radius of cylindrical tunnel,  
10 along axis  
6 along circumference of tunnel  
12 between periphery of tunnel and outer boundary of model  
*note: size keyword defines the number of zones in the grid.*

keywords for zone create:  
- dimension - edge - fill - point (boundary dimensions) - ratio (coarser toward edge) - size

## 4.2 several primitive shapes connected:

zone create radial-cylinder size 5 10 6 12 rat 1 1 1 1.2 ...  
 point 0 (0,0,0) point 1 (100,0,0) ...  
 point 2 (0,200,0) point 3 (0,0,100)  
zone create radial-tunnel size 5 10 5 12 rat 1 1 1 1.2 ...  
 point 0 (0,0,0) point 1 (0,0,-100) ...  
 point 2 (0,200,0) point 3 (100,0,0)  
; here, model boundary dimensions are 100, 200, 100  
; boundary coord are defined using point keyword  
  
zone reflect dip 90 dip-direction 270 origin (0,0,0)

this adds symmetric part.  
*note: The symmetry plane is a vertical plane (located by the dip, dip-direction, and origin keywords) coincident with the x = 0 plane. Note that dip angle (dip) and dip direction (dip-direction) assume that x corresponds to “East,” y to “North,” and z to “Up.”*

third option, the zone gridpoint create command, is available to position single points in the model region.  
*note: zone gridpoint create is used for positioning reference points of primitives*

During execution of a zone create command, a check is made for each boundary gridpoint against the boundary gridpoints of zones that already exist.  
If two boundary gridpoints fall within a tolerance of 1 ? 10-7 (relative to the magnitude of the gridpoints position vector) of each other, they are assumed to be the same point,  
If it is discovered that some gridpoints don’t match, the zone gridpoint merge command can be used to merge these gridpoints after the zone create command has been applied.

Example: (zone attach) - Two unequal sub-grids

zone create brick size 4 4 2 point 0 (0,0,0) point 1 (4,0,0) ...  
 point 2 (0,4,0) point 3 (0,0,2)  
zone create brick size 8 8 4 point 0 (0,0,2) point 1 (4,0,2) ...  
 point 2 (0,4,2) point 3 (0,0,4)  
zone attach by-face range position-z 2

Example: (zone densify)

zone create brick size 4 4 4  
zone densify segments 2 range position-x 2 4

the first two command lines can be changed to where zone densify segments 2 refines the upper zones (between the z-coordinate of 2 and 4) with the segment number of 2 on each edge.

## 4.3 Structural Element Operation

Creating a liner in the service tunnel

; liner  
structure shell create by-face range cylinder ...  
 end-1 (0,0,-1) end-2 (0,50,-1) ...  
 radius 3

The liner contains 240 structural shell elements and is connected to the FLAC3D grid at 143 structural-node links. The grid with the liner is shown below.

## 4.4 Densifying grid by specifying max size length

model new  
zone create brick size 4 4 4  
plot 'Brick' export bitmap filename 'densify3.png'  
;  
zone densify local maximum-length (0.5,0.5,0.4) range position-z 2 4  
zone attach by-face  
;  
plot 'Brick' export bitmap filename 'densify4.png'

note that in the local z-direction, the maximum size length is 0.4. FLAC3D densifies the maximum length in this direction to be 1/3 (= 0.4)  
The zone attach by-face command in this example is used to attach faces of sub-grids together rigidly to form a single grid

Always use the zone attach by-face command after the zone densify command if there are different numbers of gridpoints along faces of different zones.

### 4.4.1 Densify a grid using geometric information

model new  
zone create brick size 10 10 10  
;  
geometry set "setA" polygon create ...  
 by-positions (0,0,1) ( 5,0, 1) ( 5,10, 1) (0,10,1)  
geometry set "setA" polygon create ...  
 by-positions (5,0,1) (10,0, 5) (10,10, 5) (5,10,1)  
geometry set "setB" polygon create ...  
 by-positions (0,0,5) ( 5,0, 5) ( 5,10, 5) (0,10,5)  
geometry set "setB" polygon create ...  
 by-positions (5,0,5) (10,0,10) (10,10,10) (5,10,5)  
plot 'Brick2' export bitmap filename 'densify5.png'  
  
zone densify segments 2 range geometry-space "setA" set "setB" count 1  
zone attach by-face  
;  
plot 'Brick2' export bitmap filename 'densify6.png'

# 5 Syntax and Grammar

## 5.1 Introduction

import itasca as it  
it.command("python-reset-state false")  
it.command("""  
model new  
zone create brick size 10 10 10  
zone cmodel assign elastic  
zone property density 2950 young 12e9 poisson 0.25  
cycle 1  
""")  
it.zone.count()  
z=it.zone.find(1)  
print z  
z.pos()  
volume\_sum = 0.0  
for z in it.zone.list():  
 volume\_sum += z.vol()  
  
print volume\_sum  
print z.vol() \* it.zone.count()  
assert volume\_sum == z.vol() \* it.zone.count()  
  
z = it.zone.near ((5,5,5))  
z.pos()

## 5.2 Zones

it.zone.count() # 1000  
z = it.zone.find(1)  
for z in it.zone.list():  
 z = it.zone.near((5,5,5))  
z.pos()  
z.vol()

## 5.3 Properties

z.props() or z.props()['bulk']  
z.prop('shear')  
z.set\_prop('bulk', 8.5e9)

## 5.4 Gridpoints

gp = it.gridpoint.near((2,2,2))  
for gp in it.gridpoint.list():  
 total\_mass = gp.mass\_gravity()  
z.vol()\*z.density()\*1000

## 5.5 Structural Elements

it.structure.list()  
it.structure.find(1)  
it.structure.near((0,2,2))  
it.structure.node.find(1)  
s\_node.links()[0]

## 5.6 Extra Variables

z.set\_extra(1, 1.23)  
z.set\_extra(2, "a test string")  
z.set\_extra(1, gp.pos())

## 5.7 Groups and B.C.

if z.group("default") == "lower":  
 gp.set\_fix(0, True)  
 gp.set\_fix(1, True)  
 gp.set\_force\_load((1e6,2e6,1e6))  
it.zone.near((5,5,5)).stress()  
it.zone.near((5,5,5)).strain()  
"""

## 5.8 Parameteric Studies

"\*note: for modulus in [6e9, 8e9, 10e9, 12e9]:"  
it.command("""  
model restore 'before\_cycling'  
zone prop young {}  
model solve  
""".format(modulus))  
vertical\_disp = it.gridpoint.near((5,5,10)).disp\_z()  
print "~~~".format(modulus,vertical\_disp)

## 5.9 Results

As discussed in Reaching Equilibrium, we recommend you use the convergence 1.0 limit criteria when using the model solve command

Initially solving to a convergence of 100 or more and then examining the response is good practice. Making isosurface plots of convergence to see where the model is having trouble can give insight into where model adjustments in the interest of efficiency are best placed.

In order to determine a collapse load, it is often better to use “strain-controlled” rather than “stress-controlled” boundary conditions (i.e., apply a constant velocity and measure the reaction forces, rather than apply forces and measure displacements).

; Solve  
model solve convergence 1  
model factor-of-safety file 'slope3dfos' associated convergence 1

### 5.9.1 Measuring time of calculation

[global start = time.clock]  
model step 100  
[global rate = 10 \* zone.num / (time.clock-start) ]  
[io.out('Calculation rate = '+string(rate)+' kilo-zones/sec')]

## 5.10 Setting FISH variables

import itasca as it  
it.command('python-reset-state false')  
it.fish.set('x', 10)  
x = it.fish.get('x') yields 10

### 5.10.1 Issuing Command

import itasca as it  
import numpy as np  
data = np.loadtext('brick-data.txt')  
command\_template = ;;;   
zone create brick  
zone cmodel assign elastic  
zone property density {density} young {young} poisson {poisson}  
;;;  
density = data[0]  
young = data[1]  
poisson = data[2]  
  
command = command\_template.format(density=density, young=young, poisson=poisson)  
it.command(command)

## 5.11 String

"The value of x is {:.2f}".format(0.3872)  
"The value of x is {:.2e}".format(0.3872)  
"My name is Sasha"  
"My name is {}".format("Sasha")  
"My name is {name}".format(name="Sasha")

## 5.12 Fish Syntax

### 5.12.1 Use of …

A complete FISH statement occupies one line. However, a line may be typed across two or more lines as long as each line but the ultimate is terminated with the continuation character ( … ). Use of temporary variables as hinge points to concatenate lengthy formulas can also be handy. The following example shows how this can be done:

fish define long\_sum ;example of a sum of many things  
 local temp = v1 + v2 + v3 + v4 + v5 + v6 + v7 + v8 + v9 + v10  
 long\_sum = temp + v11 + v12 + v13 + v14 + v15  
end

### 5.12.2 Variable Types

model new  
fish define types  
 v1 = 2  
 v2 = 3.4  
 v3 = 'Have a nice day'  
 v4 = v1 \* v2  
 v5 = v3 + ', old chap'  
 v6 = vector(1,2,3)  
 v7 = matrix(vector(1,1,1))  
 v8 = true  
end  
@types  
fish list

The resulting screen display looks like this:

Name Value  
 ------- --------------------  
(function) types 0 (integer)  
 v1 2 (integer)  
 v2 3.400000000000000e+00 (real)  
 v3 'Have a nice day' (string)  
 v4 6.800000000000000e+00 (real)  
 v5 'Have a nice day, old chap' (string)  
 v6 (1.000000000000000e+00,2.000000000000000e+00,  
 3.000000000000000e+00) (vector3) [\*\*]  
 v7 3 x 1 (matrix)  
 v8 true (boolean)

### 5.12.3 Traditional for loop in FISH

standard for loop is also available in FISH to provide for additionalloop control.

fish define xxx  
 sum = 0  
 prod = 1  
 loop for (n = 1, n <= 10, n = n + 1)  
 sum = sum + n  
 prod = prod \* n  
 end\_loop  
 io.out('The sum is ' + string(sum) + ...   
 ' and the product is ' + string(prod))  
end  
@xxx

#### 5.12.3.1 Controlled loop

model new  
fish define xxx  
 sum = 0  
 prod = 1  
 loop n (1,10)  
 sum = sum + n  
 prod = prod \* n  
 end\_loop  
 io.out('The sum is ' + string(sum) + ...  
 ' and the product is ' + string(prod))  
end  
@xxx

In this case, the loop variable n is given successive values from 1 to 10, and the statements inside the loop (between the loop and endloop statements) are executed for each value. As mentioned, variable names or an arithmetic expression could be substituted for the numbers 1 or 10. Note that the exit statement can be used to break out of a FISH loop and the continue statement can be used to skip the remaining instructions in the loop, moving to the next sequence of the loop.

It is important to note that this formulation of looping is different from a for loop in most high-level programming languages. For instance, one cannot easily control the ending condition (i.e., loop from 1 to 10 excluding 10) or the incrementing mechanism (i.e., loop from 1 to 10 by twos or loop backward). A standard for loop is also available in FISH to provide for additional loop control.

### 5.12.4 if else endif construct

These statements allow conditional execution of FISH function segments; else and then are optional. The item test consists of one of the following symbols or symbol pairs:

= # > < >= <=

The displayed value of abc in this example depends on the argument provided to abc when it is executed. You should experiment with different test symbols (e.g., replace > with <).

Until now, our FISH functions have been invoked from FLAC3D, either by using the sqaure brackets [] of inline FISH, by giving the function name prepended with the the @ character, or by using the fish list command. It is also possible to do the reverse, to give FLAC3D commands from within FISH functions. Most valid FLAC3D commands can be embedded between the following FISH statements:

model new  
fish define abc(xx)  
 if xx > 0 then   
 abc = 33  
 else  
 abc = 11  
 end\_if  
end  
[abc(1)]  
[abc(-1)]

### 5.12.5 Arrays and Maps

It is often the case that one would like to store a list of objects that they will loop over in the future. These may be computed values from zones, for instance, or specific gridpoint pointers themselves. FISH has two containers to use in these circumstances, termed arrays and maps.

An array holds a list of FISH variables of any type that can be looped over or accessed by the integer index of the element of the array. Arrays can be multidimensional and do not resize dynamically. The simple example below shows how one can create an array of integers and then sum the values.

#### 5.12.5.1 Array example

model new  
fish define array\_operation  
 ;create and populate an array with products of 2  
 arr = array.create(10)  
 loop local n(1,10)  
 arr[n] = 2\*n  
 end\_loop  
   
 ;compute the sum and product of elements in the array  
 sum = 0  
 prod = 1  
 local i = 1  
 loop while (i <= array.size(arr,1))  
 sum = sum + arr[i]  
 prod = prod \* arr[i]  
 i = i + 1  
 end\_loop  
 io.out('The sum is ' + string(sum) + ...  
 ' and the product is ' + string(prod))  
end  
@array\_operation

In this example, an array is created and filled with numbers. The loop while construct is used to loop over the array entries and the sum and product are computed and output.

A map, on the other hand, is an associative container, meaning that one can access the members of a map by an integer or string used to insert a value in the map. Maps can dynamically be resized and added to one another (appending maps together), and are the preferred constructs for storing lists of FISH variables for later access.

#### 5.12.5.2 Map example

model new  
fish define map\_operation  
 ;create and populate a map with products of 2  
 my\_map = map(1,2)  
 loop local n(2,10)  
 map.add(my\_map,n,2\*n)  
 end\_loop  
   
 ;compute the sum and product of elements in the map  
 sum = 0  
 prod = 1  
 loop foreach n my\_map  
 sum = sum + n  
 prod = prod \* n  
 end\_loop  
 io.out('The sum is ' + string(sum) + ...  
 ' and the product is ' + string(prod))  
end  
@map\_operation

Unlike with arrays, maps can be looped through using the loop foreach construct. In this case, n is the value held in each map entry, not the integer name of the object in the map. Likewise, instead of using integers to insert objects into the map, one could use strings such as first, second, etc. This allows one to easily and efficiently store and access FISH variables by a user-defined name.

### 5.12.6 Fish Function

FISH functions to calculate bulk and shear moduli

model new  
fish define derive(y\_mod,p\_ratio)  
 s\_mod = y\_mod / (2.0 \* (1.0 + p\_ratio))  
 b\_mod = y\_mod / (3.0 \* (1.0 - 2.0 \* p\_ratio))  
end  
[derive(5e8,0.25)]  
[b\_mod]   
[s\_mod]

# 6 Code Block

## 6.1 Some Code

import itasca as it  
import numpy as np  
np.set\_printoptions(threshold=20)  
it.command("python-reset-state false")  
from itasca import zonearray as za  
from itasca import gridpointarray as gpa  
  
" GROUPS AND MASK ARRAYS "  
it.command("zone group \"lower\" range position-z 0 5")  
za.in\_group("lower")  
za.in\_group("lower").sum(), "zones in lower group."  
corner\_mask = reduce(np.logical\_and, (x<3, y<3, z<3))  
za.set\_group(corner\_mask, "corner", "geometry")  
print za.in\_group("corner", "geometry").sum(), "zones in corner group."  
  
" GRIDPOINTS ARRAY FUNCTIONS "  
gpos = gpa.pos()  
gx, gy, gz = gpos.T  
print gz  
f = gpa.fixity()  
print f  
f[:,][gz==0] = True, True, True  
print f  
gpa.set\_fixity(f)  
  
top\_gridpoints = gz==10  
radial\_distance = np.sqrt((gx-5)\*\*2+(gy-5)\*\*2)  
central\_gridpoints = radial\_distance < 5  
mask = np.logical\_and(top\_gridpoints, central\_gridpoints)  
print "boundary load applied to {} gridpoints".format(mask.sum())  
fapp = gpa.force\_app()  
print fapp  
fapp[:,2] = mask\*1e6\*(5.0-radial\_distance)/5.0  
gpa.set\_force\_app(fapp)  
  
print "zone centroids: "  
print za.pos()  
za.gridpoints()  
za.faces()  
za.ids()  
print za.neighbors()  
  
" =========================================== "  
" =================RESULTS=================== "  
" =========================================== "  
  
it.command("model solve")  
print "gridpoint displacements:"  
print gpa.disp()  
print "gridpoint displacement magnitudes: "  
mag = np.linalg.norm(gpa.disp(), axis=1)  
print mag  
max\_index = np.argmax(mag)  
print "Maximum displacement: {} at location {}".format(gpa.disp()[max\_index],  
 gpa.pos()[max\_index])  
  
print "Vertical displacement along the vertical line x=5, y=5: from z=0 to z=10"  
print gpa.disp()[np.logical\_and(gx==5, gy==5)][:,2]  
  
za.stress()  
  
za.stress\_flat()  
  
" =========================================== "  
" =========REFERENCE EXAMPLES================ "  
" =========================================== "  
""" Some Numpy Operation Examples  
np.array([1,2,3,4,5])  
np.linspace(0,1,15)  
np.zeros((4,4))  
a = np.linspace(0,1,15)  
b = np.ones\_like(a)  
np.sin(a)  
print a[0]  
a[0] = 20.2  
print a  
c = np.array(((1,2,3),(4,5,6),(7,8,9),(10,11,12)))  
print c  
c[0][0]  
c[:,0]  
"""  
""" SOME GRIDPOINTS EXAMPLES  
z = it.zone.near((5,5,5))  
print "central zone id: {}, position: {}".format(z.id(), z.pos())  
  
for gp in z.gridpoints():  
 print "gridpoint with id: {} at {}".format(gp.id(), gp.pos())  
"""

## 6.2 Interface

Interfaces are most often created with the zone interface create by-face command:

zone interface 'flt' create by-face separate range position-z 5  
zone interface 'flt' node property stiffness-normal 1e8 stiffness-shear 1e8

This command creates an interface named flt by separating all zone faces found at z=5 and placing interface elements and nodes on one side. Contacts are found (and forces generated) by interface nodes coming into contact with zone surface faces that are not part of the interface itself.



Figure 6.1: Code chunk syntax

Every reference to an interface uses a name (like the table command) to indicate which interface is being referred to

Interfaces in FLAC3D are one-sided objects. Interface elements are (in general) created attached to zone surface faces, which in turn create interface nodes. All contact detection is between interface nodes and zone surface faces.

Most commonly, interfaces need to be created starting with a mesh that is continuous. In that case, it is easiest to separate the mesh and create the interfaces all in one command using the separate keyword (as shown in the example above).

The new-side-origin keyword can be used to determine which side of the separation interface elements are applied to. The side opposite the location of the origin will be selected. In the example above, to select the other side, change the command to

zone interface 'flt' create by-face separate new-side-origin (0,0,10) ...  
range position-z 5

### 6.2.1 Penetration

the calculation of normal stress due to interface penetration is absolute instead of incremental. This means that moving a gridpoint relative to an interface in the normal direction will have an immediate effect on the normal stress calculated. This is not true of accumulated shear stress, which remains incremental.

In small-strain mode, gridpoints do not actually move their location in response to accumulated velocities.

small-displacement” field. is a vector field that is accumulated from the velocity field every step in small-strain mode only. For the purposes of calculating interface penetration, a gridpoint location is based on the current location plus the small-strain displacement. The smallstrain displacement may be initialized using the zone gridpoint initialize displacement-small command, and this is sometimes useful to reset the effective penetration of an interface after some grid motion. To initialize interface stresses without actually moving gridpoints, we introduce a normal stress increment that is added to the normal stress calculated from absolute penetration. It is this value that is set when the zone interface node initialize-stresses command is given. It can also be set explicitly using zone interface node stress-normal-increment.

Spatial Variation and Randomness of Property Distribution

Material properties can be specified to adjust or to vary as a function of grid position. In fact, a different property can be assigned to every zone in a FLAC3D model, regardless of model size. There are two commands avialable in FLAC3D to specfiy material properties. The first, zone property, allows multiple properties to be specified in a single command. This is convenient to completely specify properties in different regions, where that property does not vary within that region. The second can only specify one property at a time, but has optional keywords that allow the property value to be automatically varied in space. This is the zone property-distribution command. Among the available keywords are add, multiply, gradient, and vary, which can be used to provide fixed or linear variations of properties with position. For example, the following command provides a linear variation of cohesion in the x-direction:

zone property-distribution cohesion 1e6 gradient (-1e5,0,0)

An initial profile of a property can also be assigned via FISH. With FLAC3D, it is also possible to study the influence of nonhomogeneity in a material. Any type of statistical property distribution can be introduced, as each element may have a unique property value. Two optional keywords are available to apply a random distribution of a selected property with the zone propertydistribution command. The keyword deviation-gaussian assumes a normal (Gaussian) distribution for the property, with a mean value, v, and standard deviation, s. The keyword deviation-uniform assumes a uniform distribution with mean value, v, and standard deviation, s. Be careful to ensure that properties do not acquire negative values if s is large. As an example, the following command would give a mean friction angle of 40° with a standard deviation of ±5%: zone property-distribution friction 45 deviation-gaussian 2 Use of the variation keywords in any command (not just for property variation) is defined in the topic Value Modifiers (Add, Multiply, Gradient, Vary).

## 6.3 KIAST Model

import itasca as it  
import numpy as np  
np.set\_printoptions(threshold=20)  
it.command("python-reset-state false")  
from itasca import zonearray as za  
from itasca import gridpointarray as gpa  
  
# PARAMETERS #  
  
\_D\_shaft = 1  
\_H\_shaft = 7.45  
\_T\_plate = 1.5  
\_B\_footing = 3.25  
\_D\_footing = \_H\_shaft + \_T\_plate  
\_B\_soil = \_B\_footing\*5  
\_D\_soil = \_D\_footing+3  
  
\_radial = 50  
\_perimeter = 2\*\_radial  
\_axial = 2\*\_radial  
\_outer = 2\*\_radial  
  
\_bulk = 13.9e9  
\_shear = 10.4e9  
  
\_E\_o = 1e7  
\_const = 1e8  
\_poisson = 0.25  
  
# ZONE #  
  
command\_zone = """  
model new  
z crea r-t p 0 (0,0,0) ...  
 p 1 ({B\_soil},0,0) ...   
 p 2 (0,{D\_soil},0) ...  
 p 3 (0,0,{B\_soil}) ...  
 p 4 ({B\_soil},{D\_soil},0) ...  
 p 5 (0,{D\_soil},{B\_soil}) ...  
 p 6 ({B\_soil},0,{B\_soil}) ...  
 p 7 ({B\_soil},{D\_soil},{B\_soil}) ...  
 p 8 ({B\_footing},0,0) ...  
 p 9 (0,0,{B\_footing}) ...  
 p 10 ({B\_footing},{D\_soil},0) ...  
 p 11 (0,{D\_soil},{B\_footing}) ...  
 p 12 ({B\_footing},0,{B\_footing}) ...  
 p 13 ({B\_footing},{D\_soil},{B\_footing}) ...  
 size {radial} {axial} {perimeter} {outer} ...  
 rat 1 1 1 1.01 ...  
 fill  
"""  
  
command = command\_zone.format(  
B\_footing = \_B\_footing,  
B\_soil = \_B\_soil,  
D\_soil = \_D\_soil,  
radial=\_radial,  
axial = \_axial,  
perimeter = \_perimeter,  
outer = \_outer)  
  
it.command(command)  
  
# GROUP #  
  
p = za.pos()  
x,y,z = p.T  
print(it.zone.count(), "zones in whole model")  
  
shaft = reduce(np.logical\_and, (np.sqrt(x\*\*2+z\*\*2)<\_D\_shaft, y<\_H\_shaft))  
za.set\_group(shaft, "shaft") # set the zones with shaft = true have "shaft" and "geometry"  
print(za.in\_group("shaft").sum(), "zones in shaft group.") #output how many zones are in the corner group  
  
plate = reduce(np.logical\_and, (x<\_B\_footing,z<\_B\_footing, y>\_H\_shaft,y<\_D\_footing))  
za.set\_group(plate, "plate") # set the zones with plate = true have "plate" and "geometry"  
print(za.in\_group("plate").sum(), "zones in plate group.") #output how many zones are in the corner group  
  
# CONSTITUTIVE MODEL #  
  
#it.command("""  
#zone cmodel assign strain-softening range group "Radial Tunnel1"  
#zone property density 2500 bulk 2e8 shear 1e8 range group "Radial Tunnel1"  
#zone property cohesion 2e6 friction 45 tension 2e5 dilation 10 range group "Radial Tunnel1"  
#zone property table-friction 'fri' table-cohesion 'coh' table-dilation 'dil' range group "Radial Tunnel1"  
#table 'fri' add (0, 45) (.05, 42) (.1, 40) (1, 40)  
#table 'coh' add (0,2e6) (.05,1e6) (.1,5e5) (1,5e5)   
#table 'dil' add (0, 10) (.05, 3) (.1, 0)  
#""")  
  
it.command("""  
zone cmodel assign elastic range group "Radial Tunnel1"  
zone cmodel assign elastic range group 'shaft'  
zone cmodel assign elastic range group 'plate'  
  
fish define fname(E\_o,const)  
loop foreach pnt zone.list  
z\_depth = zone.pos.y(pnt)  
E = E\_o+const\*math.sqrt(z\_depth)  
zone.prop(pnt,'young')=E  
end\_loop  
end  
@fname({E\_o\_},{const\_})  
zone property poisson {poisson\_}  
plot item create zone contour property name 'young'  
""".format(E\_o\_=\_E\_o,const\_=\_const,poisson\_=\_poisson))  
  
it.command("""  
zone property bulk {bulk} shear {shear} range group 'shaft'  
zone property bulk {bulk} shear {shear} range group 'plate'  
""".format(bulk=\_bulk,shear=\_shear))  
  
#soil = za.in\_group("Radial Tunnel1")  
# list(gp.list)  
# gp.isgroup(::gp.list,"North")  
# gp.force.unbal(::ad)  
# [ad = list(gp.list)(gp.isgroup(::gp.list,"North))]

# 7 Theory

## 7.1 Interface

There are several instances in geomechanics in which it is desirable to represent planes on which sliding or separation can occur. For example:

1. joint, fault, or bedding planes in a geologic medium;
2. an interface between a foundation and the soil;
3. a contact plane between a bin or chute and the material that it contains;
4. a contact between two colliding objects; and
5. a planar “barrier” in space, which represents a fixed, non-deformable boundary at an arbitrary position and orientation.

FLAC3D provides interfaces that are characterized by Coulomb sliding and/or tensile and shear bonding. Interfaces have the properties of friction, cohesion, dilation, normal and shear stiffnesses, and tensile and shear bond strength. Although there is no restriction on the number of interfaces or the complexity of their intersections, it is generally not reasonable to model more than a few simple interfaces with FLAC3D because it is awkward to specify complicated interface geometry. The program 3DEC (Itasca 2007) is specifically designed to model many interacting bodies in three dimensions; it should be used instead of FLAC3D for the more complicated interface problems.

Interfaces may also be used to join regions that have different zone sizes. In general, the zone attach command should be used to join grids together. However, in some circumstances, it may be more convenient to use an interface for this purpose. In this case, the interface is prevented from sliding or opening because it does not correspond to any physical entity.

## 7.2 Formulation

FLAC3D represents interfaces as collections of triangular elements (interface elements), each of which is defined by three nodes (interface nodes). Interface elements can be created at any location in space. Generally, interface elements are attached to a zone surface face; two triangular interface elements are defined for every quadrilateral zone face. Interface nodes are then created automatically at every interface element vertex. When another grid surface comes into contact with an interface element, the contact is detected at the interface node and is characterized by normal and shear stiffnesses, and sliding properties.

Each interface element distributes its area to its nodes in a weighted fashion. Each interface node has an associated representative area. The entire interface is thus divided into active interface nodes representing the total area of the interface. Figure 1 illustrates the relation between interface elements and interface nodes, and the representative area associated with an individual node.



It is important to note that interfaces are one-sided in FLAC3D. (This differs from the formulation of two-sided interfaces in two-dimensional FLAC (Itasca 2011).) It may be helpful to think of FLAC3D interfaces as “shrink-wrap” that is stretched over the desired surface, causing the surface to become sensitive to interpenetration with any other face with which it may come into contact.

The fundamental contact relation is defined between the interface node and a zone surface face, also known as the target face. The normal direction of the interface force is determined by the orientation of the target face.

During each timestep, the absolute normal penetration and the relative shear velocity are calculated for each interface node and its contacting target face. Both of these values are then used by the interface constitutive model to calculate a normal force and a shear-force vector. The constitutive model is defined by a linear Coulomb shear-strength criterion that limits the shear force acting at an interface node, normal and shear stiffnesses, tensile and shear bond strengths, and a dilation angle that causes an increase in effective normal force on the target face after the shear-strength limit is reached. By default, pore pressure is used in the interface effective stress calculation. This option can be activated/deactivated using the command zone interface effective command by setting effective = on/off. Figure 2 illustrates the components of the constitutive model acting at interface node (P):



The normal and shear forces that describe the elastic interface response are determined at calculation time using the relations:

The inelastic interface logic works in the following way:

1. Bonded interface — The interface remains elastic if stresses remain below the bond strengths; there is a shear bond strength, as well as a tensile bond strength. The normal bond strength is set using the tension interface property keyword. The command zone interface node property shear-bond-ratio = sbr sets the shear bond strength to sbr times the normal bond strength. The default value of property shear-bond-ratio (if not given) is 100.0. The bond breaks if either the shear stress exceeds the shear strength, or the tensile effective normal stress exceeds the normal strength. Note that giving property shear-bond-ratio alone does not cause a bond to be established—the tensile bond strength must also be set.
2. Slip while bonded — An intact bond, by default, prevents all yield behavior (slip and separation). There is an optional property switch (bonded-slip) that causes only separation to be prevented if the bond is intact (but allows shear yield, under the control of the friction and cohesion parameters, using (F\_n) as the normal force). The command to allow/disallow slip for a bonded interface segment is zone interface node and by setting bonded-slip on or off.

The default state of bonded-slip (if not given) is off.

1. Coulomb sliding — A bond is either intact or broken. If it is broken, then the behavior of the interface segment is determined by the friction and cohesion (and of course the stiffnesses). This is the default behavior, if bond strengths are not set (zero). A broken bond segment cannot take effective tension (which may occur under compressive normal force, if the pore pressure is greater). The shear force is zero (for a nonbonded segment) if the effective normal force is tensile or zero.

The Coulomb shear-strength criterion limits the shear force by the relation:

During sliding, shear displacement may cause an increase in the effective normal stress on the joint, according to the relation:

On printout (see the zone interface node list command ) the value of tension denotes whether a bond is intact or broken (or not set) — nonzero or zero, respectively.

The normal and shear forces calculated at the interface nodes are distributed in equal and opposite directions to both the target face and the face to which the interface node is connected (the host face). Weighting functions are used to distribute the forces to the gridpoints on each face. The interface stiffnesses are added to the accumulated stiffnesses at gridpoints on both sides of the interface in order to maintain numerical stability.

Interface contacts are detected only at interface nodes, and contact forces are transferred only at interface nodes. The stress state associated with a node is assumed to be uniformly distributed over the entire representative area of the node. Interface properties are associated with each node; properties may vary from node to node.

By default, the effect of pore pressure is included in the interface calculation by using effective stress as the basis for the slip condition. (The interface pore pressure is interpolated from the target face.) This applies in model configure fluid mode, or if pore pressures are assigned with the zone water or zone gridpoint initialize pore-pressure command without specifying model configure fluid. The user can switch options for interface s by using the zone interface effective command and by setting effective on or off. By default in the FLAC3D logic, fluid flow (saturated or unsaturated) is carried across an interface, provided the interface keyword maximum-edge is not used for that particular interface. The permeable interface option can be deactivated/reactivated for interface s by using the zone interface permeability command and by setting effective on or off. Note that if the keyword maximum-edge is used after the zone interface element command, and permeability is on for a particular interface, a warning is issued to inform the user that this interface will be considered as impermeable to fluid flow. (Note that for fluid flow calculation only, a mechanical model must be present. Also, the model cycle 0 command with model mechanical active on should be used to initialize the weighting factors used to transfer fluid flow information across the interface.) No pressure drop normal to the joint and no influence of normal displacement on pore pressure is calculated.

Also, flow of fluid along the interface is not modeled.

## 7.3 Creation of Interface Geometry

Interfaces are created with the zone interface create command. For cases in which an interface between two separate grids in the model is required, the zone interface create by-face command should be used to attach an interface to one of the grid surfaces. This command generates interface elements for interface s along all surface zone faces with a center point that fall within a specified range. Any surfaces on which an interface is to be created must be generated initially; it must be possible to specify an existing surface in order to create the interface elements. A gap must be specified between two adjacent surfaces, unless the zone interface create by-face command and the separate keyword are given. In this case, the separate sub-grids may have surface gridpoints at the same location in space.

By default, two interface elements are created for each zone face. The number of interface elements can be increased by using the zone interface s element maximum-edge v command. [1] This causes all interface elements with edge lengths larger than v to subdivide into smaller elements until their lengths are smaller than v. This command can be used to increase the resolution and decrease arching of forces in portions of a model that have large contrasts in zone size across an interface.

Several rules should be followed when using interface elements in FLAC3D:

1. If a smaller surface area contacts a larger surface area (e.g., a small block resting on a large block), the interface should be attached to the smaller region.
2. If there is a difference in zone density between two adjacent grids, the interface should be attached to the grid with the greater zone density (i.e., the greater number of zones within the same area).
3. The size of interface elements should always be equal to or smaller than the target faces with which they will come into contact. If this is not the case, the interface elements should be subdivided into smaller elements.
4. Interface elements should be limited to grid surfaces that will actually come into contact with another grid.  
   A simple example illustrating the procedure for interface creation is provided in “DippingJoint.f3dat.” The corresponding project file, “DippingJoint.f3prj,” is located in the folder “datafiles InterfaceDippingJoint.” The example is a block specimen containing a single joint dipping at an angle of

; Create interface elements on the top surface of the base   
zone interface 'joint' create by-face separate range group 'Top' group 'Base'  
model save 'int1'  
return

## 7.4 Typical Properties



Post-Failure Properties In many instances, particularly in mining engineering, the response of a material after failure has initiated is an important factor in the engineering design. Consequently, the post-failure behavior must be simulated in the material model. In FLAC3D, this is accomplished with properties that define four types of post failure response: 1. shear dilatancy; 2. shear hardening/softening; 3. volumetric hardening/softening; and 4. tensile softening. These properties are only activated after failure is initiated, as defined by the Mohr-Coulomb relation or the tensile-failure criterion. Shear dilatancy is simulated with the Mohr-Coulomb, ubiquitous-joint and strain-softening MohrCoulomb and ubiquitous-joint models. Shear hardening/softening is simulated with the strain-softening Mohr-Coulomb and ubiquitous-joint models, and volumetric hardening/softening is simulated with the modified Cam-clay model. Tensile softening is simulated with the strain-softening Mohr-Coulomb and ubiquitous-joint models


### 7.4.1 Shear Dilatancy

 Shear dilatancy, or dilatancy, is the change in volume that occurs with shear distortion of a material. Dilatancy is characterized by a dilation angle, , which is related to the ratio of plastic volume change to plastic shear strain. This angle can be specified in the Mohr-Coulomb ubiquitous-joint and strain-hardening/ softening models in FLAC3D. Dilation angle is typically determined from triaxial tests or shear-box tests. For example, the idealized relation for dilatancy, based upon the Mohr-Coulomb failure surface, is depicted for a triaxial test in the figure below. The dilation angle is found from the plot of volumetric strain versus axial strain. Note that the initial slope for this plot corresponds to the elastic regime, while the slope used to measure the dilation angle corresponds to the plastic regime  Selected Strength Properties (drained, laboratory-scale) for Soils (Ortiz et al. 1980)



### 7.4.2 Compression Test on strain-softening material

model new  
; Create zones  
zone create cylinder point 0 (0,0,0) point 1 (1,0,0) point 2 (0,2,0) ...  
point 3 (0,0,1) size 4 5 4  
zone reflect normal (1,0,0)  
zone reflect normal (0,0,1)  
; Constitutive Model and properties  
zone cmodel assign strain-softening  
zone property bulk 1.19e10 shear 1.1e10  
zone property cohesion 2.72e5 friction 44 tension 2e5  
zone property table-cohesion 'coh' table-friction 'fri'  
table 'coh' add (0,2.72e5) (1e-4,2e5) (2e-4,1.5e5) (3e-4,1.03e5) (1,1.03e5)  
table 'fri' add (0,44) (1e-4,42) (2e-4,40) (3e-4,38) (1,38)  
; Boundary Conditions  
zone face apply velocity (0, 1e-7,0) range position-y 0  
zone face apply velocity (0,-1e-7,0) range position-y 2  
; Histories  
zone history displacement-y position (0,0,0)  
zone history stress-yy position (0,1,0)  
zone history stress-yy position (1,1,0)  
model step 3000  
model save 'Softening'

The horizontal stress-displacement response is monitored again, as shown in the image below. This test produces distinct peak and residual failure stress levels 

The strain-softening model assumes both a brittle softening (due to reduction in cohesion) and a gradual softening (due to a reduction in friction angle). The selection of the properties is discussed further in Material Properties. Comparison of the two images above illustrates the different responses of the two models. The initial response up to the onset of failure is identical, but postfailure behavior is quite different. Clearly, more data are required to use the strain-softening model and, typically, the softening model must be calibrated for each specific problem.

# 8 Command

## 8.1 Interface

### 8.1.1 zone face group

zone face group s keyword …

Example:   
  
```python  
zone face group 'wall' internal range group 'wall-c' group 'pile'

Adds a group name ‘wall’ to zone faces included in the optional range. Also can be used with zone face group “slotname = groupname” Zone face may belong to many groups, up to 128. keywords: internal, or, remove.  
- internal: to select all faces.  
If specified, then the range looks at internal faces as well as surface faces.

* or: considered inside the surface if any of those conditions has a non-null model.
* remove: group is removed from the zone face.

### 8.1.2 zone face skin

zone face skin

Generates contiguous face groups by skinning.

“skinning” refers to automatic face group generation, which occurs as follows: the program looks for contiguous faces and puts them into automatically named groups within the slot named skin. Two faces are not considered contiguous if the angle between two faces exceeds the break angle, or if the two faces belong to different groups according to the command’s slot specification. Unless internal is specified, the operation of zone face skin is restricted to external faces. Only zone faces that have no zone on the other side, a hidden zone on the other side are considered surface faces. When use-hidden-zones is used, within specified range will be included for consideration.

group names are generated as follows: sEast, sWest, sNorth, sSouth, sTop, sBottom

Internal faces are assigned names of the group on either side that changed in order to create them.

### 8.1.3 zone separate

zone separete by-face new-side group 'iwall' slot 'int' range group 'wall' or 'base'

separates internal faces specified by the range. The gridpoints of the face are duplicated, and new face is created. New faces and gridpoints get copies of all group and extra variable assignments belonging to the original face and gridpoint.

Example: If Fred and George are group names assigned to zones, then

range group 'Fred' group 'George'

will select faces that are connected to zone of both group Fred and George.

keyword: - by-face: attempts to separate all internal faces in the range - new-side group: newly created faces will be assigned the group name in the specified slot. The default slot, is named Default.

### 8.1.4 zone interface create

zone interface 'side' create by-face range group 'wall' and 'iwall'  
  
zone interface 'side' node property stiffness-normal 1e8 stiffness-shear 1e8 friction 20 cohesion 30000

creates nodes or elements on interface side

There are two techniques for creating an interface. 1. To derive an interface from a range of zone faces using by-face keyword. 2. To specify a triangular interface element from 3 points. 3. Command may also be used to construct an interface node that may be used with the element keyword.

keyword: - by-face: interface elements are created on all surface zone faces that are within the specified range. An error will occur if interface elements from that interface already exist on the selected faces. If the optional separate keyword is used, then internal zone faces are selected by the range. The list of selected faces is then automatically separated (as with zone separate) and interface elements placed on one side. The following are for the separate keyword: new-side-origin, clear-attach.

* element point i keyword … : create a triangular interface element by specifying 3 points. Three verticies must be specified by the following keyword. Each point can be created and located in space using the position keyword, or an existing interface node with ID i may be specified. The interface element that is created is not attached to a grid face even if the location corresponds to that of the face. the element is fixed in space. The active side of the element is defined by walking around the edge of the element, from point 1 to point 2 to point 3; the active side is up when walking in a clockwise direction.

For each point of the element, one of the following two keywords must be supplied: node i, position v.

* node v : this creates an interface node at position v. If a node already exists at the selected location, an error is reported. The created node is fixed in space.

# (APPENDIX) Appendix

# 9 1. Template

## 9.1 Problem Description

## 9.2 Modeling Procedure

## 9.3 Zones/Groups

## 9.4 Properties

## 9.5 B.C. and I.C.

## 9.6 Initial Equilibrium

## 9.7 Alterations

## 9.8 Results

# 10 Reference Collective

### 10.0.1 Uplift Resistance of Anchor Plate

#### 10.0.1.1 Before 1968

* Coulomb
* Mohr
* Kotter’s equation
* Balla (1961)
* Mors
* Matsuo

#### 10.0.1.2 Post-1968

* Meyerhof, G.G., and Adams, J.I. 1968
* Meyerhof, G.G. 1973
* Das, B.M., and Seeley, G.R. 1975
* Rowe, R.K., and Davis, H. 1982
* Dickin, E.A., and Leung, C.F. 1983
* Murray, E.J., and Geddes, J.D. 1987
* Dickin, E.A. 1988
* Koutsabeloulis, N.C., and Griffiths, D.V. 1989 #### Post-2000
* Merifield, R.S., and Sloan, S.W. 2006

### 10.0.2 Numerical Analysis

### 10.0.3 Standards

* IEEE 2001
* DS 1110, DS 1111

### 10.0.4 Textbook

* Das, B. M. 2013. Earth Anchors

### 10.0.5 Ph.D Thesis

### 10.0.6 Award Lecture